February 1996

  Appendix A:



          Projection Transformation Package Projection Parameters

  -----------------------------------------------------------------------------
                          |       		Array Element                    |
   Code & Projection Id   |----------------------------------------------------
                          |   1  |   2  |  3   |  4   |   5   |    6    |7 | 8|
  -----------------------------------------------------------------------------
   0 Geographic           |      |      |      |      |       |         |  |  |
   1 U T M                |Lon/Z |Lat/Z |      |      |       |         |  |  |
   2 State Plane          |      |      |      |      |       |         |  |  |
   3 Albers Equal Area    |SMajor|SMinor|STDPR1|STDPR2|CentMer|OriginLat|FE|FN|
   4 Lambert Conformal C  |SMajor|SMinor|STDPR1|STDPR2|CentMer|OriginLat|FE|FN|
   5 Mercator             |SMajor|SMinor|      |      |CentMer|TrueScale|FE|FN|
   6 Polar Stereographic  |SMajor|SMinor|      |      |LongPol|TrueScale|FE|FN|
   7 Polyconic            |SMajor|SMinor|      |      |CentMer|OriginLat|FE|FN|
   8 Equid. Conic A       |SMajor|SMinor|STDPAR|      |CentMer|OriginLat|FE|FN|
     Equid. Conic B       |SMajor|SMinor|STDPR1|STDPR2|CentMer|OriginLat|FE|FN|
   9 Transverse Mercator  |SMajor|SMinor|Factor|      |CentMer|OriginLat|FE|FN|
  10 Stereographic        |Sphere|      |      |      |CentLon|CenterLat|FE|FN|
  11 Lambert Azimuthal    |Sphere|      |      |      |CentLon|CenterLat|FE|FN|
  12 Azimuthal            |Sphere|      |      |      |CentLon|CenterLat|FE|FN|
  13 Gnomonic             |Sphere|      |      |      |CentLon|CenterLat|FE|FN|
  14 Orthographic         |Sphere|      |      |      |CentLon|CenterLat|FE|FN|
  15 Gen. Vert. Near Per  |Sphere|      |Height|      |CentLon|CenterLat|FE|FN|
  16 Sinusoidal           |Sphere|      |      |      |CentMer|         |FE|FN|
  17 Equirectangular      |Sphere|      |      |      |CentMer|TrueScale|FE|FN|
  18 Miller Cylindrical   |Sphere|      |      |      |CentMer|         |FE|FN|
  19 Van der Grinten      |Sphere|      |      |      |CentMer|OriginLat|FE|FN|
  20 Hotin Oblique Merc A |SMajor|SMinor|Factor|      |       |OriginLat|FE|FN|
     Hotin Oblique Merc B |SMajor|SMinor|Factor|AziAng|AzmthPt|OriginLat|FE|FN|
  21 Robinson             |Sphere|      |      |      |CentMer|         |FE|FN|
  22 Space Oblique Merc A |SMajor|SMinor|      |IncAng|AscLong|         |FE|FN|
     Space Oblique Merc B |SMajor|SMinor|Satnum|Path  |       |         |FE|FN|
  23 Alaska Conformal     |SMajor|SMinor|      |      |       |         |FE|FN|
  24 Interrupted Goode    |Sphere|      |      |      |       |         |  |  |
  25 Mollweide            |Sphere|      |      |      |CentMer|         |FE|FN|
  26 Interrupt Mollweide  |Sphere|      |      |      |       |         |  |  |
  27 Hammer               |Sphere|      |      |      |CentMer|         |FE|FN|
  28 Wagner IV            |Sphere|      |      |      |CentMer|         |FE|FN|
  29 Wagner VII           |Sphere|      |      |      |CentMer|         |FE|FN|
  30 Oblated Equal Area   |Sphere|      |Shapem|Shapen|CentLon|CenterLat|FE|FN|
  -----------------------------------------------------------------------------
  
  Array elements 9-15 Continued on page 2


    Projection Transformation Package Projection Parameters elements 9-15
    continued from page 1:

	 ---------------------------------------------------------
       	                   	 	|      Array Element       |
	  Code & Projection Id		|---------------------------
	  		         	|  9  | 10 |  11 | 12 | 13 |  
	 ---------------------------------------------------------
	  0 Geographic		 	|     |    |     |    |    |
	  1 U T M	      	 	|     |    |     |    |    |
	  2 State Plane	 	|     |    |     |    |    |
	  3 Albers Equal Area	 	|     |    |     |    |    |
	  4 Lambert Conformal C 	|     |    |     |    |    |
	  5 Mercator		 	|     |    |     |    |    |
	  6 Polar Stereographic  	|     |    |     |    |    |
	  7 Polyconic		 	|     |    |     |    |    |
	  8 Equid. Conic A       	|zero |    |     |    |    |   
	    Equid. Conic B	 	|one  |    |     |    |    |
	  9 Transverse Mercator  	|     |    |     |    |    |
	 10 Stereographic	 	|     |    |     |    |    |
	 11 Lambert Azimuthal    	|     |    |     |    |    |    
	 12 Azimuthal            	|     |    |     |    |    |    
	 13 Gnomonic 		 	|     |    |     |    |    |
	 14 Orthographic	 	|     |    |     |    |    |
	 15 Gen. Vert. Near Per  	|     |    |     |    |    |
	 16 Sinusoidal           	|     |    |     |    |    |
	 17 Equirectangular	 	|     |    |     |    |    |
	 18 Miller Cylindrical   	|     |    |     |    |    |
	 19 Van der Grinten	 	|     |    |     |    |    |
	 20 Hotin Oblique Merc A 	|Long1|Lat1|Long2|Lat2|zero|   
 	    Hotin Oblique Merc B 	|     |    |     |    |one |
	 21 Robinson    	 	|     |    |     |    |    |
	 22 Space Oblique Merc A 	|PSRev|LRat|PFlag|    |zero|    
	    Space Oblique Merc B 	|     |    |     |    |one |
	 23 Alaska Conformal     	|     |    |     |    |    |
	 24 Interrupted Goode    	|     |    |     |    |    |
	 25 Mollweide		 	|     |    |     |    |    |
	 26 Interrupt Mollweide  	|     |    |     |    |    |
	 27 Hammer		 	|     |    |     |    |    |
	 28 Wagner IV		 	|     |    |     |    |    |
	 29 Wagner VII		 	|     |    |     |    |    |
	 30 Oblated Equal Area   	|Angle|    |     |    |    |
	 ---------------------------------------------------------

  where 
      Lon/Z 	 Longitude of any point in the UTM zone or zero.  If zero,
		 a zone code must be specified.
      Lat/Z	 Latitude of any point in the UTM zone or zero.  If zero, a
		 zone code must be specified.
      SMajor    Semi-major axis of ellipsoid.  If zero, Clarke 1866 in meters
		 is assumed.
      SMinor    Eccentricity squared of the ellipsoid if less than zero,
		 if zero, a spherical form is assumed, or if greater than
		 zero, the semi-minor axis of ellipsoid.
      Sphere    Radius of reference sphere.  If zero, 6370997 meters is used.
      STDPAR    Latitude of the standard parallel
      STDPR1    Latitude of the first standard parallel
      STDPR2    Latitude of the second standard parallel
      CentMer   Longitude of the central meridian
      OriginLat Latitude of the projection origin
      FE    	 False easting in the same units as the semi-major axis
      FN    	 False northing in the same units as the semi-major axis
      TrueScale Latitude of true scale
      LongPol   Longitude down below pole of map
      Factor    Scale factor at central meridian (Transverse Mercator) or
		 center of projection (Hotine Oblique Mercator)
      CentLon   Longitude of center of projection
      CenterLat Latitude of center of projection
      Height    Height of perspective point
      Long1	 Longitude of first point on center line (Hotine Oblique
		 Mercator, format A)
      Long2	 Longitude of second point on center line (Hotine Oblique
		 Mercator, format A)
      Lat1	 Latitude of first point on center line (Hotine Oblique
		 Mercator, format A)
      Lat2	 Latitude of second point on center line (Hotine Oblique
		 Mercator, format A)
      AziAng    Azimuth angle east of north of center line (Hotine Oblique
		 Mercator, format B)
      AzmthPt   Longitude of point on central meridian where azimuth occurs
		 (Hotine Oblique Mercator, format B)
      IncAng    Inclination of orbit at ascending node, counter-clockwise
		 from equator (SOM, format A)
      AscLong   Longitude of ascending orbit at equator (SOM, format A)
      PSRev	 Period of satellite revolution in minutes (SOM, format A)
      LRat	 Landsat ratio to compensate for confusion at northern end
		 of orbit (SOM, format A -- use 0.5201613)
      PFlag	 End of path flag for Landsat:  0 = start of path,
		 1 = end of path (SOM, format A)
      Satnum    Landsat Satellite Number (SOM, format B)
      Path	 Landsat Path Number (Use WRS-1 for Landsat 1, 2 and 3 and
		 WRS-2 for Landsat 4, 5 and 6.)  (SOM, format B)
      Shapem	 Oblated Equal Area oval shape parameter m
      Shapen	 Oblated Equal Area oval shape parameter n
      Angle	 Oblated Equal Area oval rotation angle



                                   NOTES

   Array elements 14 and 15 are set to zero
   All array elements with blank fields are set to zero
   All angles (latitudes, longitudes, azimuths, etc.) are entered in packed
 	degrees/ minutes/ seconds (DDDMMMSSS.SS) format

   The following notes apply to the Space Oblique Mercator A projection.

      A portion of Landsat rows 1 and 2 may also be seen as parts of rows
   246 or 247.  To place these locations at rows 246 or 247, set the end of
   path flag (parameter 11) to 1--end of path.  This flag defaults to zero.

      When Landsat-1,2,3 orbits are being used, use the following values
   for the specified parameters:

      Parameter 4   099005031.2
      Parameter 5   128.87 degrees - (360/251 * path number) in packed
		    DMS format
      Parameter 9   103.2669323
      Parameter 10  0.5201613

      When Landsat-4,5 orbits are being used, use the following values
   for the specified parameters:

      Parameter 4   098012000.0
      Parameter 5   129.30 degrees - (360/233 * path number) in packed
		    DMS format
      Parameter 9   98.884119
      Parameter 10  0.5201613
































					4
